-- VHDL Entity Morse_test.charToMorseController_tester.interface
--
-- Created:
--          by - axel.amand.UNKNOWN (WE7860)
--          at - 14:50:43 28.04.2023
--
-- Generated by Mentor Graphics' HDL Designer(TM) 2019.2 (Build 5)
--
LIBRARY ieee;
  USE ieee.std_logic_1164.all;
  USE ieee.numeric_std.ALL;

ENTITY charToMorseController_tester IS
    GENERIC( 
        clockFrequency : real;
        characterBitNb : positive
    );
    PORT( 
        morseOut     : IN     std_ulogic;
        readChar     : IN     std_ulogic;
        char         : OUT    std_ulogic_vector (characterBitNb-1 DOWNTO 0);
        charNotReady : OUT    std_ulogic;
        clock        : OUT    std_ulogic;
        reset        : OUT    std_ulogic
    );

-- Declarations

END charToMorseController_tester ;

