# -------------------------------------------------------------------------- #
#
# Copyright (C) 2019  Intel Corporation. All rights reserved.
# Your use of Intel Corporation's design tools, logic functions 
# and other software and tools, and any partner logic 
# functions, and any output files from any of the foregoing 
# (including device programming or simulation files), and any 
# associated documentation or information are expressly subject 
# to the terms and conditions of the Intel Program License 
# Subscription Agreement, the Intel Quartus Prime License Agreement,
# the Intel FPGA IP License Agreement, or other applicable license
# agreement, including, without limitation, that your use is for
# the sole purpose of programming logic devices manufactured by
# Intel and sold by Intel or its authorized distributors.  Please
# refer to the applicable agreement for further details, at
# https://fpgasoftware.intel.com/eula.
#
# -------------------------------------------------------------------------- #
#
# Quartus Prime
# Version 18.1.1 Build 646 04/11/2019 SJ Lite Edition
# Date created = 21:29:54  June 08, 2021
#
# -------------------------------------------------------------------------- #
#
# Notes:
#
# 1) The default values for assignments are stored in the file:
#		de0-nano-test-setup_assignment_defaults.qdf
#    If this file doesn't exist, see file:
#		assignment_defaults.qdf
#
# 2) Altera recommends that you do not modify this file. This
#    file is updated automatically by the Quartus Prime software
#    and any changes you make may be lost or overwritten.
#
# -------------------------------------------------------------------------- #


set_global_assignment -name FAMILY "Cyclone IV E"
set_global_assignment -name DEVICE EP4CE22F17C6
set_global_assignment -name TOP_LEVEL_ENTITY neorv32_ProcessorTop_Test
set_global_assignment -name ORIGINAL_QUARTUS_VERSION 20.1.0
set_global_assignment -name PROJECT_CREATION_TIME_DATE "16:40:53  APRIL 10, 2021"
set_global_assignment -name LAST_QUARTUS_VERSION "18.1.1 Lite Edition"
set_global_assignment -name PROJECT_OUTPUT_DIRECTORY output_files
set_global_assignment -name MIN_CORE_JUNCTION_TEMP 0
set_global_assignment -name MAX_CORE_JUNCTION_TEMP 85
set_global_assignment -name ERROR_CHECK_FREQUENCY_DIVISOR 1
set_global_assignment -name POWER_PRESET_COOLING_SOLUTION "23 MM HEAT SINK WITH 200 LFPM AIRFLOW"
set_global_assignment -name POWER_BOARD_THERMAL_MODEL "NONE (CONSERVATIVE)"
set_global_assignment -name PARTITION_NETLIST_TYPE SOURCE -section_id neorv32_ProcessorTop_Test
set_global_assignment -name PARTITION_FITTER_PRESERVATION_LEVEL PLACEMENT_AND_ROUTING -section_id neorv32_ProcessorTop_Test
set_global_assignment -name PARTITION_COLOR 16764057 -section_id neorv32_ProcessorTop_Test
set_location_assignment PIN_R8 -to clk_i
set_location_assignment PIN_J15 -to rstn_i
set_location_assignment PIN_C3 -to uart0_txd_o
set_location_assignment PIN_A3 -to uart0_rxd_i
set_location_assignment PIN_L3 -to gpio_o[7]
set_location_assignment PIN_B1 -to gpio_o[6]
set_location_assignment PIN_F3 -to gpio_o[5]
set_location_assignment PIN_D1 -to gpio_o[4]
set_location_assignment PIN_A11 -to gpio_o[3]
set_location_assignment PIN_B13 -to gpio_o[2]
set_location_assignment PIN_A13 -to gpio_o[1]
set_location_assignment PIN_A15 -to gpio_o[0]
set_global_assignment -name QSYS_FILE neorv32_test_qsys.qsys
set_global_assignment -name QIP_FILE ../neorv32_qsys_component/neorv32_qsys.qip
set_global_assignment -name VHDL_FILE ../../../rtl/core/neorv32_application_image.vhd
set_global_assignment -name VHDL_FILE ../../../rtl/core/neorv32_bootloader_image.vhd
set_global_assignment -name VHDL_FILE ./../../../rtl/core/neorv32_dmem.entity.vhd -library neorv32
set_global_assignment -name VHDL_FILE ./../../../rtl/core/neorv32_imem.entity.vhd -library neorv32
set_global_assignment -name VHDL_FILE ./../../../rtl/core/mem/neorv32_dmem.default.vhd -library neorv32
set_global_assignment -name VHDL_FILE ./../../../rtl/core/mem/neorv32_imem.default.vhd -library neorv32
set_global_assignment -name VHDL_FILE neorv32_ProcessorTop_Test.vhd
set_instance_assignment -name PARTITION_HIERARCHY root_partition -to | -section_id neorv32_ProcessorTop_Test